# Static Call Graph - [AutoGuideStick\AutoGuideStick.axf]

# Static Call Graph for image AutoGuideStick\AutoGuideStick.axf

#<CALLGRAPH># ARM Linker, 6210000: Last Updated: Sun Jun 8 22:25:39 2025

### Maximum Stack Usage = 568 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config

### Functions with no stack information

- _tx_initialize_low_level
- __tx_BadHandler
- __tx_IntHandler
- SysTick_Handler
- __tx_NMIHandler
- __tx_DBGHandler
- _tx_thread_schedule
- PendSV_Handler
- _tx_vfp_access
- _tx_thread_stack_build
- _tx_timer_interrupt

### Mutually Recursive functions

- SecureFault_Handler ⇒ SecureFault_Handler
- SVC_Handler ⇒ SVC_Handler
- ADC1_IRQHandler ⇒ ADC1_IRQHandler

  ### Function Pointers

  - ADC1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - ADC2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - BusFault_Handler from stm32h5xx_it.o(.text.BusFault_Handler) referenced from startup_stm32h563xx.o(RESET)
  - CEC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - CORDIC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - CRS_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - DAC1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - DCACHE1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - DCMI_PSSI_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - DTS_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - DebugMon_Handler from stm32h5xx_it.o(.text.DebugMon_Handler) referenced from startup_stm32h563xx.o(RESET)
  - ETH_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI10_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI11_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI12_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI13_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI14_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI15_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI7_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI8_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - EXTI9_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FDCAN1_IT0_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FDCAN1_IT1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FDCAN2_IT0_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FDCAN2_IT1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FLASH_S_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FMAC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FMC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - FPU_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel0_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA1_Channel7_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel0_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GPDMA2_Channel7_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - GTZC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - HASH_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - HardFault_Handler from stm32h5xx_it.o(.text.HardFault_Handler) referenced from startup_stm32h563xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C4_ER_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I2C4_EV_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I3C1_ER_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - I3C1_EV_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - ICACHE_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - IWDG_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPTIM1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPTIM2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPTIM3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPTIM4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPTIM5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPTIM6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - LPUART1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - MemManage_Handler from stm32h5xx_it.o(.text.MemManage_Handler) referenced from startup_stm32h563xx.o(RESET)
  - NMI_Handler from stm32h5xx_it.o(.text.NMI_Handler) referenced from startup_stm32h563xx.o(RESET)
  - OCTOSPI1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - PVD_AVD_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - PendSV_Handler from tx_thread_schedule.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - RAMCFG_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - RCC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - RCC_S_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - RNG_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - RTC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - RTC_S_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - Reset_Handler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SAI2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SDMMC1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SDMMC2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SVC_Handler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SecureFault_Handler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SysTick_Handler from tx_initialize_low_level.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - SystemInit from system_stm32h5xx.o(.text.SystemInit) referenced from startup_stm32h563xx.o(.text)
  - TAMP_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM12_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM13_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM14_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM15_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM16_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM17_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM1_UP_IRQHandler from stm32h5xx_it.o(.text.TIM1_UP_IRQHandler) referenced from startup_stm32h563xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART12_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART4_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART5_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART7_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART8_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART9_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UART_DMAAbortOnError from stm32h5xx_hal_uart.o(.text.UART_DMAAbortOnError) referenced 2 times from stm32h5xx_hal_uart.o(.text.HAL_UART_IRQHandler)
  - UCPD1_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - USART10_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - USART11_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - USART1_IRQHandler from stm32h5xx_it.o(.text.USART1_IRQHandler) referenced from startup_stm32h563xx.o(RESET)
  - USART2_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - USART3_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - USART6_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - USB_DRD_FS_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - UsageFault_Handler from stm32h5xx_it.o(.text.UsageFault_Handler) referenced from startup_stm32h563xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32h563xx.o(.text) referenced from startup_stm32h563xx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32h563xx.o(.text)
  - _tx_thread_shell_entry from tx_thread_shell_entry.o(.text._tx_thread_shell_entry) referenced 2 times from tx_thread_create.o(.text._tx_thread_create)
  - _tx_thread_timeout from tx_thread_timeout.o(.text._tx_thread_timeout) referenced 2 times from tx_thread_create.o(.text._tx_thread_create)
  - _tx_timer_thread_entry from tx_timer_thread_entry.o(.text._tx_timer_thread_entry) referenced 2 times from tx_timer_initialize.o(.text._tx_timer_initialize)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(.text)

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 84 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_loop (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, __scatter.o(!!handler_null), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000034))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000010))

  __rt_lib_init_relocate_pie_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000035))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000027))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 568 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SecureFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Calls]

  - >> SecureFault_Handler
  [Called By]
  - >> SecureFault_Handler
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Calls]

  - >> ADC1_IRQHandler
  [Called By]
  - >> ADC1_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(RESET)

  ADC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  CEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  CORDIC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  CRS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  DAC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  DCACHE1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  DCMI_PSSI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  DTS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  EXTI9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FDCAN1_IT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FDCAN1_IT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FDCAN2_IT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FDCAN2_IT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FLASH_S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FMAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GPDMA2_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  GTZC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  HASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C4_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I2C4_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I3C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  I3C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  ICACHE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  IWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPTIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPTIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPTIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPTIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPTIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  LPUART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  OCTOSPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  PVD_AVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  RAMCFG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  RCC_S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  RTC_S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SAI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SDMMC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SDMMC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UART12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UART9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  UCPD1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  USART10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  USART11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  USB_DRD_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  __user_initial_stackheap (Thumb, 10 bytes, Stack size 0 bytes, startup_stm32h563xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  _tx_initialize_low_level (Thumb, 0 bytes, Stack size unknown bytes, tx_initialize_low_level.o(.text))
  [Called By]

  - >> _tx_initialize_kernel_enter

  __tx_BadHandler (Thumb, 0 bytes, Stack size unknown bytes, tx_initialize_low_level.o(.text), UNUSED)
  [Calls]

  - >> __tx_BadHandler
  [Called By]
  - >> __tx_BadHandler

  __tx_IntHandler (Thumb, 0 bytes, Stack size unknown bytes, tx_initialize_low_level.o(.text), UNUSED)

  SysTick_Handler (Thumb, 0 bytes, Stack size unknown bytes, tx_initialize_low_level.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = SysTick_Handler ⇒ _tx_timer_interrupt ⇒ _tx_timer_expiration_process ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_timer_interrupt
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(RESET)

  __tx_NMIHandler (Thumb, 0 bytes, Stack size unknown bytes, tx_initialize_low_level.o(.text), UNUSED)
  [Calls]

  - >> __tx_NMIHandler
  [Called By]
  - >> __tx_NMIHandler

  __tx_DBGHandler (Thumb, 0 bytes, Stack size unknown bytes, tx_initialize_low_level.o(.text), UNUSED)
  [Calls]

  - >> __tx_DBGHandler
  [Called By]
  - >> __tx_DBGHandler

  _tx_thread_schedule (Thumb, 0 bytes, Stack size unknown bytes, tx_thread_schedule.o(.text))
  [Called By]

  - >> _tx_initialize_kernel_enter

  PendSV_Handler (Thumb, 0 bytes, Stack size unknown bytes, tx_thread_schedule.o(.text))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  _tx_vfp_access (Thumb, 0 bytes, Stack size unknown bytes, tx_thread_schedule.o(.text), UNUSED)

  _tx_thread_stack_build (Thumb, 0 bytes, Stack size unknown bytes, tx_thread_stack_build.o(.text))
  [Called By]

  - >> _tx_thread_create

  _tx_timer_interrupt (Thumb, 0 bytes, Stack size unknown bytes, tx_timer_interrupt.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = _tx_timer_interrupt ⇒ _tx_timer_expiration_process ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_thread_time_slice
  - >> _tx_timer_expiration_process
  [Called By]
  - >> SysTick_Handler

  __aeabi_uldivmod (Thumb, 0 bytes, Stack size 48 bytes, lludivv7m.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = __aeabi_uldivmod
  [Called By]
  - >> UART_SetConfig

  _ll_udiv (Thumb, 240 bytes, Stack size 48 bytes, lludivv7m.o(.text), UNUSED)

  __aeabi_memset (Thumb, 16 bytes, Stack size 0 bytes, aeabi_memset.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memset ⇒ _memset ⇒ _memset_w
  [Calls]
  - >> _memset
  [Called By]
  - >> _tx_thread_create

  __aeabi_memclr (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr.o(.text), UNUSED)

  __rt_memclr (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr.o(.text), UNUSED)

  _memset (Thumb, 64 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _memset ⇒ _memset_w
  [Calls]
  - >> _memset_w
  [Called By]
  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text))
  [Called By]

  - >> SystemClock_Config
  - >> _tx_byte_pool_create
  - >> _tx_timer_initialize
  - >> _tx_thread_initialize
  - >> _tx_thread_create

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text))
  [Called By]

  - >> HAL_UART_MspInit

  __rt_memclr_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 74 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _memset_w
  [Called By]
  - >> _memset

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  App_ThreadX_Init (Thumb, 14 bytes, Stack size 8 bytes, app_threadx.o(.text.App_ThreadX_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = App_ThreadX_Init
  [Called By]
  - >> tx_application_define

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h5xx_it.o(.text.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32h5xx_it.o(.text.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  Error_Handler (Thumb, 6 bytes, Stack size 0 bytes, main.o(.text.Error_Handler))
  [Called By]

  - >> HAL_UART_MspInit
  - >> MX_USART1_UART_Init
  - >> SystemClock_Config

  HAL_DMA_Abort (Thumb, 278 bytes, Stack size 24 bytes, stm32h5xx_hal_dma.o(.text.HAL_DMA_Abort))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_DMA_Abort
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_Abort_IT (Thumb, 84 bytes, Stack size 8 bytes, stm32h5xx_hal_dma.o(.text.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_GPIO_Init (Thumb, 746 bytes, Stack size 20 bytes, stm32h5xx_hal_gpio.o(.text.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit

  HAL_GetTick (Thumb, 12 bytes, Stack size 0 bytes, stm32h5xx_hal.o(.text.HAL_GetTick))
  [Called By]

  - >> RCCEx_PLL3_Config
  - >> RCCEx_PLL2_Config
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCC_OscConfig
  - >> UART_WaitOnFlagUntilTimeout
  - >> UART_CheckIdleState
  - >> HAL_DMA_Abort

  HAL_IncTick (Thumb, 26 bytes, Stack size 0 bytes, stm32h5xx_hal.o(.text.HAL_IncTick))
  [Called By]

  - >> HAL_TIM_PeriodElapsedCallback

  HAL_Init (Thumb, 94 bytes, Stack size 16 bytes, stm32h5xx_hal.o(.text.HAL_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 206 bytes, Stack size 56 bytes, stm32h5xx_hal_timebase_tim.o(.text.HAL_InitTick))
  [Stack]

  - Max Depth = 120
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_TIM_Base_Start_IT
  - >> HAL_TIM_Base_Init
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetClockConfig
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32h5xx_hal_msp.o(.text.HAL_MspInit))
  [Called By]

  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 20 bytes, Stack size 16 bytes, stm32h5xx_hal_cortex.o(.text.HAL_NVIC_EnableIRQ))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_NVIC_EnableIRQ ⇒ __NVIC_EnableIRQ
  [Calls]
  - >> __NVIC_EnableIRQ
  [Called By]
  - >> HAL_InitTick
  - >> HAL_UART_MspInit

  HAL_NVIC_SetPriority (Thumb, 46 bytes, Stack size 32 bytes, stm32h5xx_hal_cortex.o(.text.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> __NVIC_SetPriority
  - >> NVIC_EncodePriority
  - >> __NVIC_GetPriorityGrouping
  [Called By]
  - >> HAL_InitTick
  - >> HAL_UART_MspInit

  HAL_NVIC_SetPriorityGrouping (Thumb, 16 bytes, Stack size 16 bytes, stm32h5xx_hal_cortex.o(.text.HAL_NVIC_SetPriorityGrouping))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_NVIC_SetPriorityGrouping ⇒ __NVIC_SetPriorityGrouping
  [Calls]
  - >> __NVIC_SetPriorityGrouping
  [Called By]
  - >> HAL_Init

  HAL_RCCEx_GetPLL1ClockFreq (Thumb, 748 bytes, Stack size 36 bytes, stm32h5xx_hal_rcc_ex.o(.text.HAL_RCCEx_GetPLL1ClockFreq))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_RCCEx_GetPLL1ClockFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCCEx_GetPLL2ClockFreq (Thumb, 748 bytes, Stack size 36 bytes, stm32h5xx_hal_rcc_ex.o(.text.HAL_RCCEx_GetPLL2ClockFreq))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_RCCEx_GetPLL2ClockFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCCEx_GetPLL3ClockFreq (Thumb, 748 bytes, Stack size 36 bytes, stm32h5xx_hal_rcc_ex.o(.text.HAL_RCCEx_GetPLL3ClockFreq))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_RCCEx_GetPLL3ClockFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCCEx_GetPeriphCLKFreq (Thumb, 10488 bytes, Stack size 120 bytes, stm32h5xx_hal_rcc_ex.o(.text.HAL_RCCEx_GetPeriphCLKFreq))
  [Stack]

  - Max Depth = 172
  - Call Chain = HAL_RCCEx_GetPeriphCLKFreq ⇒ HAL_RCC_GetPCLK3Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCCEx_GetPLL3ClockFreq
  - >> HAL_RCCEx_GetPLL2ClockFreq
  - >> HAL_RCCEx_GetPLL1ClockFreq
  - >> HAL_RCC_GetPCLK3Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> UART_SetConfig

  HAL_RCCEx_PeriphCLKConfig (Thumb, 6382 bytes, Stack size 184 bytes, stm32h5xx_hal_rcc_ex.o(.text.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 208
  - Call Chain = HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> RCCEx_PLL3_Config
  - >> RCCEx_PLL2_Config
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_MspInit

  HAL_RCC_ClockConfig (Thumb, 1172 bytes, Stack size 32 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 152
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_GetTick
  - >> HAL_InitTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetClockConfig (Thumb, 108 bytes, Stack size 12 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_GetClockConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_RCC_GetClockConfig
  [Called By]
  - >> HAL_InitTick

  HAL_RCC_GetHCLKFreq (Thumb, 52 bytes, Stack size 8 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> HAL_RCC_GetPCLK3Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_OscConfig

  HAL_RCC_GetPCLK1Freq (Thumb, 38 bytes, Stack size 8 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCC_GetPCLK2Freq (Thumb, 38 bytes, Stack size 8 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> HAL_InitTick

  HAL_RCC_GetPCLK3Freq (Thumb, 38 bytes, Stack size 8 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_GetPCLK3Freq))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_RCC_GetPCLK3Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq

  HAL_RCC_GetSysClockFreq (Thumb, 700 bytes, Stack size 36 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_RCC_OscConfig (Thumb, 2556 bytes, Stack size 40 bytes, stm32h5xx_hal_rcc.o(.text.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 160
  - Call Chain = HAL_RCC_OscConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_GetTick
  - >> HAL_InitTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 154 bytes, Stack size 8 bytes, stm32h5xx_hal_cortex.o(.text.HAL_SYSTICK_CLKSourceConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_CLKSourceConfig
  [Called By]
  - >> HAL_Init

  HAL_TIMEx_Break2Callback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_Break2Callback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_Break2Callback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_BreakCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_BreakCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_BreakCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_CommutCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_CommutCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_DirectionChangeCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_DirectionChangeCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_DirectionChangeCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_EncoderIndexCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_EncoderIndexCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_EncoderIndexCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_IndexErrorCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_IndexErrorCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_IndexErrorCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_TransitionErrorCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim_ex.o(.text.HAL_TIMEx_TransitionErrorCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIMEx_TransitionErrorCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_Base_Init (Thumb, 168 bytes, Stack size 16 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> TIM_Base_SetConfig
  - >> HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_InitTick

  HAL_TIM_Base_MspInit (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 402 bytes, Stack size 12 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_Base_Start_IT))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIM_Base_Start_IT
  [Called By]
  - >> HAL_InitTick

  HAL_TIM_IC_CaptureCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_IC_CaptureCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIM_IC_CaptureCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 768 bytes, Stack size 24 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback
  [Calls]
  - >> HAL_TIMEx_TransitionErrorCallback
  - >> HAL_TIMEx_IndexErrorCallback
  - >> HAL_TIMEx_DirectionChangeCallback
  - >> HAL_TIMEx_EncoderIndexCallback
  - >> HAL_TIMEx_CommutCallback
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIMEx_Break2Callback
  - >> HAL_TIMEx_BreakCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_PeriodElapsedCallback
  [Called By]
  - >> TIM1_UP_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_OC_DelayElapsedCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIM_OC_DelayElapsedCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_PWM_PulseFinishedCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIM_PWM_PulseFinishedCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 34 bytes, Stack size 16 bytes, main.o(.text.HAL_TIM_PeriodElapsedCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_PeriodElapsedCallback
  [Calls]
  - >> HAL_IncTick
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_tim.o(.text.HAL_TIM_TriggerCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_TIM_TriggerCallback
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_UARTEx_DisableFifoMode (Thumb, 124 bytes, Stack size 12 bytes, stm32h5xx_hal_uart_ex.o(.text.HAL_UARTEx_DisableFifoMode))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_UARTEx_DisableFifoMode
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UARTEx_RxEventCallback (Thumb, 12 bytes, Stack size 8 bytes, stm32h5xx_hal_uart.o(.text.HAL_UARTEx_RxEventCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UARTEx_RxEventCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_UARTEx_RxFifoFullCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_uart_ex.o(.text.HAL_UARTEx_RxFifoFullCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_UARTEx_RxFifoFullCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_UARTEx_SetRxFifoThreshold (Thumb, 140 bytes, Stack size 24 bytes, stm32h5xx_hal_uart_ex.o(.text.HAL_UARTEx_SetRxFifoThreshold))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_UARTEx_SetRxFifoThreshold ⇒ UARTEx_SetNbDataToProcess
  [Calls]
  - >> UARTEx_SetNbDataToProcess
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UARTEx_SetTxFifoThreshold (Thumb, 140 bytes, Stack size 24 bytes, stm32h5xx_hal_uart_ex.o(.text.HAL_UARTEx_SetTxFifoThreshold))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_UARTEx_SetTxFifoThreshold ⇒ UARTEx_SetNbDataToProcess
  [Calls]
  - >> UARTEx_SetNbDataToProcess
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UARTEx_TxFifoEmptyCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_uart_ex.o(.text.HAL_UARTEx_TxFifoEmptyCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_UARTEx_TxFifoEmptyCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_UARTEx_WakeupCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_uart_ex.o(.text.HAL_UARTEx_WakeupCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_UARTEx_WakeupCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_UART_ErrorCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_uart.o(.text.HAL_UART_ErrorCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_UART_ErrorCallback
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 1346 bytes, Stack size 64 bytes, stm32h5xx_hal_uart.o(.text.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_UART_IRQHandler ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_UARTEx_RxFifoFullCallback
  - >> HAL_UARTEx_TxFifoEmptyCallback
  - >> HAL_UARTEx_WakeupCallback
  - >> HAL_UARTEx_RxEventCallback
  - >> HAL_UART_ErrorCallback
  - >> UART_EndTransmit_IT
  - >> UART_EndRxTransfer
  - >> HAL_DMA_Abort
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 170 bytes, Stack size 16 bytes, stm32h5xx_hal_uart.o(.text.HAL_UART_Init))
  [Stack]

  - Max Depth = 536 + Unknown Stack Size
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_CheckIdleState
  - >> UART_SetConfig
  - >> UART_AdvFeatureConfig
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 192 bytes, Stack size 312 bytes, usart.o(.text.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 520 + Unknown Stack Size
  - Call Chain = HAL_UART_MspInit ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_NVIC_SetPriority
  - >> HAL_GPIO_Init
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> Error_Handler
  - >> __aeabi_memclr8
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_TxCpltCallback (Thumb, 8 bytes, Stack size 4 bytes, stm32h5xx_hal_uart.o(.text.HAL_UART_TxCpltCallback))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_UART_TxCpltCallback
  [Called By]
  - >> UART_EndTransmit_IT

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h5xx_it.o(.text.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  MX_GPIO_Init (Thumb, 66 bytes, Stack size 8 bytes, gpio.o(.text.MX_GPIO_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = MX_GPIO_Init
  [Called By]
  - >> main

  MX_ThreadX_Init (Thumb, 8 bytes, Stack size 8 bytes, app_threadx.o(.text.MX_ThreadX_Init))
  [Stack]

  - Max Depth = 272 + Unknown Stack Size
  - Call Chain = MX_ThreadX_Init ⇒ _tx_initialize_kernel_enter ⇒ _tx_initialize_high_level ⇒ _tx_timer_initialize ⇒ _tx_thread_create ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_initialize_kernel_enter
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 142 bytes, Stack size 16 bytes, usart.o(.text.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 552 + Unknown Stack Size
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> HAL_UARTEx_DisableFifoMode
  - >> HAL_UARTEx_SetRxFifoThreshold
  - >> HAL_UARTEx_SetTxFifoThreshold
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h5xx_it.o(.text.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  NMI_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h5xx_it.o(.text.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  SystemClock_Config (Thumb, 198 bytes, Stack size 120 bytes, main.o(.text.SystemClock_Config))
  [Stack]

  - Max Depth = 280 + Unknown Stack Size
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_OscConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority ⇒ NVIC_EncodePriority
  [Calls]
  - >> HAL_RCC_ClockConfig
  - >> Error_Handler
  - >> HAL_RCC_OscConfig
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 310 bytes, Stack size 8 bytes, system_stm32h5xx.o(.text.SystemInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(.text)

  TIM1_UP_IRQHandler (Thumb, 16 bytes, Stack size 8 bytes, stm32h5xx_it.o(.text.TIM1_UP_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM1_UP_IRQHandler ⇒ HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(RESET)

  TIM_Base_SetConfig (Thumb, 858 bytes, Stack size 12 bytes, stm32h5xx_hal_tim.o(.text.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  UART_AdvFeatureConfig (Thumb, 328 bytes, Stack size 4 bytes, stm32h5xx_hal_uart.o(.text.UART_AdvFeatureConfig))
  [Stack]

  - Max Depth = 4
  - Call Chain = UART_AdvFeatureConfig
  [Called By]
  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 326 bytes, Stack size 40 bytes, stm32h5xx_hal_uart.o(.text.UART_CheckIdleState))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout ⇒ UART_EndRxTransfer
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_UART_Init

  UART_SetConfig (Thumb, 1048 bytes, Stack size 48 bytes, stm32h5xx_hal_uart.o(.text.UART_SetConfig))
  [Stack]

  - Max Depth = 220
  - Call Chain = UART_SetConfig ⇒ HAL_RCCEx_GetPeriphCLKFreq ⇒ HAL_RCC_GetPCLK3Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> __aeabi_uldivmod
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 268 bytes, Stack size 32 bytes, stm32h5xx_hal_uart.o(.text.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_WaitOnFlagUntilTimeout ⇒ UART_EndRxTransfer
  [Calls]
  - >> HAL_GetTick
  - >> UART_EndRxTransfer
  [Called By]
  - >> UART_CheckIdleState

  USART1_IRQHandler (Thumb, 16 bytes, Stack size 8 bytes, stm32h5xx_it.o(.text.USART1_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32h563xx.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32h5xx_it.o(.text.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32h563xx.o(RESET)

  _tx_byte_pool_create (Thumb, 304 bytes, Stack size 64 bytes, tx_byte_pool_create.o(.text._tx_byte_pool_create))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _tx_byte_pool_create
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> _txe_byte_pool_create

  _tx_initialize_high_level (Thumb, 134 bytes, Stack size 8 bytes, tx_initialize_high_level.o(.text._tx_initialize_high_level))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = _tx_initialize_high_level ⇒ _tx_timer_initialize ⇒ _tx_thread_create ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_timer_initialize
  - >> _tx_thread_initialize
  [Called By]
  - >> _tx_initialize_kernel_enter

  _tx_initialize_kernel_enter (Thumb, 104 bytes, Stack size 16 bytes, tx_initialize_kernel_enter.o(.text._tx_initialize_kernel_enter))
  [Stack]

  - Max Depth = 264 + Unknown Stack Size
  - Call Chain = _tx_initialize_kernel_enter ⇒ _tx_initialize_high_level ⇒ _tx_timer_initialize ⇒ _tx_thread_create ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> tx_application_define
  - >> _tx_initialize_low_level
  - >> _tx_thread_schedule
  - >> _tx_initialize_high_level
  [Called By]
  - >> MX_ThreadX_Init

  _tx_thread_create (Thumb, 538 bytes, Stack size 80 bytes, tx_thread_create.o(.text._tx_thread_create))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = _tx_thread_create ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_thread_system_preempt_check
  - >> _tx_thread_system_resume
  - >> _tx_thread_stack_build
  - >> __aeabi_memclr4
  - >> __aeabi_memset
  [Called By]
  - >> _tx_timer_initialize

  _tx_thread_initialize (Thumb, 126 bytes, Stack size 16 bytes, tx_thread_initialize.o(.text._tx_thread_initialize))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = _tx_thread_initialize
  [Calls]
  - >> __aeabi_memclr4
  [Called By]
  - >> _tx_initialize_high_level

  _tx_thread_shell_entry (Thumb, 148 bytes, Stack size 40 bytes, tx_thread_shell_entry.o(.text._tx_thread_shell_entry))
  [Stack]

  - Max Depth = 188
  - Call Chain = _tx_thread_shell_entry ⇒ _tx_thread_system_suspend ⇒ _tx_timer_system_activate
  [Calls]
  - >> _tx_thread_system_suspend
  [Address Reference Count : 1]
  - tx_thread_create.o(.text._tx_thread_create)

  _tx_thread_system_preempt_check (Thumb, 112 bytes, Stack size 28 bytes, tx_thread_system_preempt_check.o(.text._tx_thread_system_preempt_check))
  [Stack]

  - Max Depth = 28
  - Call Chain = _tx_thread_system_preempt_check
  [Called By]
  - >> _txe_byte_pool_create
  - >> _tx_thread_create

  _tx_thread_system_resume (Thumb, 584 bytes, Stack size 96 bytes, tx_thread_system_resume.o(.text._tx_thread_system_resume))
  [Stack]

  - Max Depth = 112
  - Call Chain = _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_timer_system_deactivate
  [Called By]
  - >> _tx_timer_expiration_process
  - >> _tx_thread_timeout
  - >> _tx_thread_create

  _tx_thread_system_suspend (Thumb, 640 bytes, Stack size 120 bytes, tx_thread_system_suspend.o(.text._tx_thread_system_suspend))
  [Stack]

  - Max Depth = 148
  - Call Chain = _tx_thread_system_suspend ⇒ _tx_timer_system_activate
  [Calls]
  - >> _tx_timer_system_activate
  [Called By]
  - >> _tx_timer_thread_entry
  - >> _tx_thread_shell_entry

  _tx_thread_time_slice (Thumb, 162 bytes, Stack size 20 bytes, tx_thread_time_slice.o(.text._tx_thread_time_slice))
  [Stack]

  - Max Depth = 20
  - Call Chain = _tx_thread_time_slice
  [Called By]
  - >> _tx_timer_interrupt

  _tx_thread_timeout (Thumb, 114 bytes, Stack size 48 bytes, tx_thread_timeout.o(.text._tx_thread_timeout))
  [Stack]

  - Max Depth = 160
  - Call Chain = _tx_thread_timeout ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_thread_system_resume
  [Address Reference Count : 1]
  - tx_thread_create.o(.text._tx_thread_create)

  _tx_timer_expiration_process (Thumb, 60 bytes, Stack size 24 bytes, tx_timer_expiration_process.o(.text._tx_timer_expiration_process))
  [Stack]

  - Max Depth = 136
  - Call Chain = _tx_timer_expiration_process ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> _tx_thread_system_resume
  [Called By]
  - >> _tx_timer_interrupt

  _tx_timer_initialize (Thumb, 286 bytes, Stack size 48 bytes, tx_timer_initialize.o(.text._tx_timer_initialize))
  [Stack]

  - Max Depth = 240 + Unknown Stack Size
  - Call Chain = _tx_timer_initialize ⇒ _tx_thread_create ⇒ _tx_thread_system_resume ⇒ _tx_timer_system_deactivate
  [Calls]
  - >> __aeabi_memclr4
  - >> _tx_thread_create
  [Called By]
  - >> _tx_initialize_high_level

  _tx_timer_system_activate (Thumb, 212 bytes, Stack size 28 bytes, tx_timer_system_activate.o(.text._tx_timer_system_activate))
  [Stack]

  - Max Depth = 28
  - Call Chain = _tx_timer_system_activate
  [Called By]
  - >> _tx_thread_system_suspend
  - >> _tx_timer_thread_entry

  _tx_timer_system_deactivate (Thumb, 112 bytes, Stack size 16 bytes, tx_timer_system_deactivate.o(.text._tx_timer_system_deactivate))
  [Stack]

  - Max Depth = 16
  - Call Chain = _tx_timer_system_deactivate
  [Called By]
  - >> _tx_thread_system_resume

  _tx_timer_thread_entry (Thumb, 536 bytes, Stack size 104 bytes, tx_timer_thread_entry.o(.text._tx_timer_thread_entry))
  [Stack]

  - Max Depth = 252
  - Call Chain = _tx_timer_thread_entry ⇒ _tx_thread_system_suspend ⇒ _tx_timer_system_activate
  [Calls]
  - >> _tx_thread_system_suspend
  - >> _tx_timer_system_activate
  [Address Reference Count : 1]
  - tx_timer_initialize.o(.text._tx_timer_initialize)

  _txe_byte_pool_create (Thumb, 372 bytes, Stack size 80 bytes, txe_byte_pool_create.o(.text._txe_byte_pool_create))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = _txe_byte_pool_create ⇒ _tx_byte_pool_create
  [Calls]
  - >> _tx_byte_pool_create
  - >> _tx_thread_system_preempt_check
  [Called By]
  - >> tx_application_define

  main (Thumb, 32 bytes, Stack size 16 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 568 + Unknown Stack Size
  - Call Chain = main ⇒ MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_RCCEx_PeriphCLKConfig ⇒ RCCEx_PLL3_Config
  [Calls]
  - >> MX_ThreadX_Init
  - >> MX_USART1_UART_Init
  - >> MX_GPIO_Init
  - >> SystemClock_Config
  - >> HAL_Init
  [Called By]
  - >> __rt_entry_main

  tx_application_define (Thumb, 88 bytes, Stack size 24 bytes, app_azure_rtos.o(.text.tx_application_define))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = tx_application_define ⇒ _txe_byte_pool_create ⇒ _tx_byte_pool_create
  [Calls]
  - >> _txe_byte_pool_create
  - >> App_ThreadX_Init
  [Called By]
  - >> _tx_initialize_kernel_enter

  _fp_init (Thumb, 26 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  __NVIC_SetPriorityGrouping (Thumb, 60 bytes, Stack size 12 bytes, stm32h5xx_hal_cortex.o(.text.__NVIC_SetPriorityGrouping))
  [Stack]

  - Max Depth = 12
  - Call Chain = __NVIC_SetPriorityGrouping
  [Called By]
  - >> HAL_NVIC_SetPriorityGrouping

  __NVIC_GetPriorityGrouping (Thumb, 16 bytes, Stack size 0 bytes, stm32h5xx_hal_cortex.o(.text.__NVIC_GetPriorityGrouping))
  [Called By]

  - >> HAL_NVIC_SetPriority

  NVIC_EncodePriority (Thumb, 108 bytes, Stack size 32 bytes, stm32h5xx_hal_cortex.o(.text.NVIC_EncodePriority))
  [Stack]

  - Max Depth = 32
  - Call Chain = NVIC_EncodePriority
  [Called By]
  - >> HAL_NVIC_SetPriority

  __NVIC_SetPriority (Thumb, 66 bytes, Stack size 8 bytes, stm32h5xx_hal_cortex.o(.text.__NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = __NVIC_SetPriority
  [Called By]
  - >> HAL_NVIC_SetPriority

  __NVIC_EnableIRQ (Thumb, 48 bytes, Stack size 4 bytes, stm32h5xx_hal_cortex.o(.text.__NVIC_EnableIRQ))
  [Stack]

  - Max Depth = 4
  - Call Chain = __NVIC_EnableIRQ
  [Called By]
  - >> HAL_NVIC_EnableIRQ

  RCCEx_PLL2_Config (Thumb, 364 bytes, Stack size 24 bytes, stm32h5xx_hal_rcc_ex.o(.text.RCCEx_PLL2_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCCEx_PLL2_Config
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCCEx_PeriphCLKConfig

  RCCEx_PLL3_Config (Thumb, 364 bytes, Stack size 24 bytes, stm32h5xx_hal_rcc_ex.o(.text.RCCEx_PLL3_Config))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCCEx_PLL3_Config
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCCEx_PeriphCLKConfig

  UART_EndRxTransfer (Thumb, 158 bytes, Stack size 16 bytes, stm32h5xx_hal_uart.o(.text.UART_EndRxTransfer))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_EndRxTransfer
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> UART_WaitOnFlagUntilTimeout

  UART_DMAAbortOnError (Thumb, 30 bytes, Stack size 16 bytes, stm32h5xx_hal_uart.o(.text.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 20
  - Call Chain = UART_DMAAbortOnError ⇒ HAL_UART_ErrorCallback
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32h5xx_hal_uart.o(.text.HAL_UART_IRQHandler)

  UART_EndTransmit_IT (Thumb, 68 bytes, Stack size 16 bytes, stm32h5xx_hal_uart.o(.text.UART_EndTransmit_IT))
  [Stack]

  - Max Depth = 20
  - Call Chain = UART_EndTransmit_IT ⇒ HAL_UART_TxCpltCallback
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UARTEx_SetNbDataToProcess (Thumb, 138 bytes, Stack size 8 bytes, stm32h5xx_hal_uart_ex.o(.text.UARTEx_SetNbDataToProcess))
  [Stack]

  - Max Depth = 8
  - Call Chain = UARTEx_SetNbDataToProcess
  [Called By]
  - >> HAL_UARTEx_SetRxFifoThreshold
  - >> HAL_UARTEx_SetTxFifoThreshold

  ### Undefined Global Symbols